# Reverse DNS

## Get PTR record

PTR records refer to a parent device: either a Cloud Server or a Cloud Load Balancer with a public virtual IP address. You must supply a fully formed resource object in order to retrieve either one’s PTR record:

    /** @param $parent OpenCloud\DNS\Resource\HasPtrRecordsInterface */

    $ptr = $service->ptrRecord(array(
        'parent' => $parent
    ));

So, in the above example, the `$parent` object could be an instance of `OpenCloud\Compute\Resource\Server` or `OpenCloud\LoadBalancer\Resource\LoadBalancer` - because they both implement `OpenCloud\DNS\Resource\HadPtrRecordsInterface`. Please consult the server documentation and load balancer documentation for more detailed usage instructions.

## List PTR records

    /** @param $parent OpenCloud\DNS\Resource\HasPtrRecordsInterface */

    $ptrRecords = $service->ptrRecordList($parent);

    foreach ($ptrRecords as $ptrRecord) {

    }

## Add PTR record

    $parent = $computeService->server('foo-server-id');

    $ptr = $dnsService->ptrRecord(array(
        'parent' => $parent,
        'ttl'    => 3600,
        'name'   => 'example.com',
        'type'   => 'PTR',
        'data'   => '192.0.2.7'
    ));

    $ptr->create();

Here is a table that explains the above attributes:

Name | Description | Required
--- | --- | ---
type | Specifies the record type as “PTR”. | Yes
name | Specifies the name for the domain or subdomain. Must be a valid domain name. | Yes
data | The data field for PTR records must be a valid IPv4 or IPv6 IP address. | Yes
ttl | If specified, must be greater than 300. Defaults to 3600 if no TTL is specified. | No
comment | If included, its length must be less than or equal to 160 characters. | No

## Modify PTR record

    $ptr->update(array(
        'ttl' => $ptr->ttl * 2
    ));

## Delete PTR record

    $ptr->delete();